Block 4 of 12- March Block Required for Drawing

|  |  |  |
| --- | --- | --- |
| A | B | A |
| C |
| B |

12” Finished Block

F

D

G

E

E

G

F

D

|  |  |  |
| --- | --- | --- |
| A | 2 | 2 ½” x 8 ½” rectangles |
| B | 2 | 2 ½” x 4 ½” rectangles |
| C | 1 | 4 ½” square |
| D | 2 | 2 ½” x 6 ½” rectangles |
| E | 2 | 2 ½” x 4½” rectangles |
| F | 2 | 2 ½” x 6 ½” rectangles |
| G | 2 | 2 ½” x 4½” rectangles |

*Piecing Instructions*

Assemble Inner Box C, B blocks on top and bottom

|  |
| --- |
| B |

|  |
| --- |
| C |

|  |
| --- |
| B |

Complete assembly of A blocks on left and right sides

|  |
| --- |
| A |

|  |
| --- |
| A |

|  |
| --- |
| B |
| C |
| B |

Assemble F/D and E/G for final top, bottom and sides:

D

F

F

D

G

E

E

G

Assemble F/D strip to top and bottom

F

D

|  |  |  |
| --- | --- | --- |
| A | B | A |
| C |
| B |

D

F

Complete block assembly with attaching E/G strips to left and right sides

E

F

D

|  |  |  |
| --- | --- | --- |
| A | B | A |
| C |
| B |

G

G

E

F

D